The DTMF repeater module, is used to retransmit received DTMF digits. This can
be used to control other remote stations that is also DTMF controlled. All
entered DTMF digits will be retransmitted and ignored completely by SvixLink.

De-activate the module by sending the number sign for at least three seconds.
