The propagation monitor receive propagation alerts from VHF DX dot net. These are announced by
voice messages as soon as they are received.

The types of messages announced are: sporadic e, au-rora and troppo opening.
