This is the SvixLink system. It is a multi purpose voice services system for ham
radio use. The system is controlled by DTMF commands. All commands consists of
one or more digits ended with the number sign.

Pressing the star key will make the system identify itself.

The system is divided into several modules which has its own purpose. You
activate a module by sending its module i d ended with the number sign. Most
modules will play their help message if sending command 0 when its activated.
